**TEXTILES COMMITTEE**

(Ministry of Textiles, Government of India)

Administration (Housekeeping)

P. Balu Road, Prabhadevi, Mumbai- 400 025

Email. [tchkmumbai@gmail.com](mailto:tchkmumbai@gmail.com)

Web Site. [www.textilescommittee.nic.in](http://www.textilescommittee.nic.in)

Tel: 022-66527523/586/532

No.51/17/2008-AD Vol.VI 18th December, 2017

To,

As per list

**Sub:- Inviting bids for making of ramp for Divyang (handicap) persons at Textiles Committee, Prabhadevi, Mumbai**

Sir,

Textiles Committee, Government of India, Ministry of Textiles invites bids for making of ramp for Divyang (handicap) persons at Textiles Committee, Prabhadevi, Mumbai. **Two options are available to bidders for executing the work related to Ramp i.e. either 1) Wooden flooring ramp or 2) Granite flooring ramp. Bidders are requested to submit the details either in one or both options. (Please refer Selection Criteria at Sr. No.7, A & B & Annexure-I for detailed specification).**

**The Terms & Conditions are as under**:

1. The bid shall be on letter-head of the bidder and submitted in a sealed cover supercribing “Making of ramp for Divyang (handicap) persons at Textiles Committee, Prabhadevi, Mumbai” on or before 09.01.2018 at 3.00 PM
2. **EMD** : Interest free EMD of Rs.2000/- by way of Demand Draft to be submitted along with bid. Non submission of requiste EMD shall reject the bid. The EMD of unsuccessful bidders shall be returned back with 45 days after selection of successful bidder. EMD shall be forfeited incase of alteration of quoted rates and/ or non acceptance of work order after selection.
3. **Performance Security**: The successful bidder shall deposit 5% of total value of contract with Textiles Committee by way of DD as interest free security deposit. In case of non satisfactory performance or breach of contracts the performance security @ 5% so deposited with Textiles Committee shall be forfeited.

Cont…2

:2:

1. **The design of proposed work is enclosed only for reference/ explanatory purpose.** **The rates shall only be quoted on actual site visit.**
2. The bidder shall visit Textiles Committee for inspection & measurement at site before due date & time only.
3. Textiles Committee shall not be responsible for any delay in receipt of bid or non-receipt of bid sent by post/ courier. The bidders shall submit the bid by post/ courier/ hand delivery in the Admn-HK division of Textiles Committee, Mumbai on or before the due date.
4. **Selection criteria:**
5. Only L-1 Bidder shall be selected for award of contract in either one option (any one option only). Textiles Committee reserves the right to select the either option (any one option only) after receipt & opening of Bids.
6. Textiles Committee reserves the right to award the contract to Lowest Bidder No.2 and/ or No.3 in case the Lowest Bidder No.1 backs out of the contract. In such a case, the EMD of Lowest Bidder No.1 shall be forfeited. It is also at the liberty of Textiles Committee to ask the Lowest Bidder No. 2 and/ or 3 in succeeding order to carry out the scope of work under the contract at the rates quoted by Lowest Bidder No.1. In succeeding order if L-2 and/or L-3 rejects/ fails to accept the offer then fresh bids will be called.
7. Textiles Committee has the right to accept or reject all or particular bid at any time without assigning any reason thereof.
8. **Payment Terms:** The payment will be made on satisfactory completion of work as per the specification contained in the work order and within the time as stipulated in work order. No advance payment.
9. No damage shall be caused to the property of Textiles Committee while carrying out the assigned work. Any damage to property of Textiles Committee shall be recovered from the selected bidder in terms of money or replacement of said property.
10. The work should be carried out within 30 days at the said site of Textiles Committee, at Prabhadevi, Mumbai at the said cost after receipt of Work Order.
11. The bid should be on actual site visit as per design enclosed.
12. **The bid in sealed cover supercribed “Making of Ramp for Divyang (handicap) persons at Textiles Committee, Prabhadevi, Mumbai” shall be submitted to the Assistant Director (HK), Textiles Committee, P. Balu Road, Prabhadevi, Mumbai 400 025, on or before 09.01.2018 at 3.00 PM opening of bids on 09.01.2018 at 5.00 PM.**
13. **Note: - Design is enclosed for reference / explanatory purpose only & rates shall be quoted on actual site visit only.**

Yours faithfully,

(Ganesh Bangar)

Assistant Director (EPQA & Admn-HK)

**Annexure-I**

**Bids for making of Ramp shall be submitted in the below format only.**

**< On letter head >**

Ref. No. Date:

To,

The Secretary,

Textiles Committee,

P. Balu Marg,

Prabhadevi,

Mumbai – 400 025.

**Sub. :-** Submissionof bids for the making of Ramp at Estate of Textiles Committee ,Prabhadevi, Mumbai.

Dear Sir,

We are pleased to give our bids for making of Ramp at Estate Textiles Committee, Prabhadevi are as below.

**Option A**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Specification for wooden flooring ramp** | | | | | |
| Sr. No. | Description | QTY | Unit | Rate | Amount  in Rs. |
| 1 | Ramp platform in – Sagwan (साग का लकड़ा) |  |  |  |  |
| 2 | Ramp stand material – either in wood/ M.S/ iron ( as selected by party) |  |  |  |  |
| 3 | Ramp Ralling – Stainless Steel Material |  |  |  |  |
| **Civil work:** | | | | | |
| 1 | Dismantling/ Demolition to level the Ramp to the ground for size L-37inch x W-47 inch |  |  |  |  |
| **Total in Rs. (inclusive tax if any) for option A** | |  |  |  |  |
| **In word (Rupees )** | | | | | |

**Cont…2**

**:2:**

**Option B**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Specification for granite flooring ramp** | | | | | |
| Sr. No. | Description | QTY | Unit | Rate | Amount  in Rs. |
| 1 | Scrapping of existing flooring for greeping the new brick work. |  |  |  |  |
| 2 | Brick work in 1:6 proportions at one side of the ramp in 9 inch thick. |  |  |  |  |
| 3 | Wall plastering of 12mm thick at vertical surface of the wall |  |  |  |  |
| 4 | M-10 PCC of 4 inch thick below flooring |  |  |  |  |
| 5 | Granite vertical dado at one side of the ramp which maintain the existing architecheral design. |  |  |  |  |
| 6 | Rough Grenite flooring with non slippery surface for ramp which maintain the tactile paving (hatching lines) at every 6 inch interval to maintain design and proper slope over sand bedding upto 35 mm thick |  |  |  |  |
| **Total in Rs.(inclusive tax if any) for option B** | |  |  |  |  |
| **In word (Rupees. )** | | | | | |

We hereby confirm that the rates quoted above shall remain valid & constant for the period of one year from placing of work order.

Thanking you.

Yours faithfully,

**Signature & stamp of Authorised signatory of bidder**

**along with company seal**